Bio Radio SDK - Xamarin Android: GLNeuroTech.Devices.BioRadio.Configuration Namespace Reference

| Bio Radio SDK - Xamarin Android

Classes | Enumerations
GLNeuroTech.Devices.BioRadio.Configuration Namespace Reference

## Classes

class | AuxiliaryChannelConfiguration
| Describes the configuration of a Auxiliary channel. More...
class | BioPotentialChannelConfiguration
| Bio Potential Channel Configuration - inherit from Channel Configuration More...
class | BioRadioConfiguration
| The BioRadioConfiguration class encapsulates all settings that can be defined and programmed for the BioRadio. More...
class | BioRadioConfigurationJavaScriptConverter
| Bio Radio Configuration - Java Script Converter (JsonConvereter) More...
class | ChannelConfiguration
| This class describes all settings that apply across all device channels. More...
class | ChannelConfigurationFactory
class | EnumHelper
class | EventMarkerChannelConfiguration
| Represents the configuration of a BioRadio event marker channel. More...
class | MemsChannelConfiguration
| Describes the configuration applied to the internal MEMS sensor of the BioRadio device. More...
class | NotConnectedExternalSensorConfiguration
| Represents the configuration for an external sensor that is not actually connected. This is intended as a helper class to indicate that there is no sensor at a particular index. More...
class | PulseOxChannelConfiguration
| Describes the configuration of a PulseOx PulseOx channel. More...

## Enumerations

enum | AuxiliaryTransducerType : ushort { AuxiliaryTransducerType.BloodPressure = 0, AuxiliaryTransducerType.FlowRate = 1, AuxiliaryTransducerType.ForcePlate = 2, AuxiliaryTransducerType.GripStrength = 3, AuxiliaryTransducerType.Temperature = 4 }
| The list of transducers that can be selected for the Auxiliary port of a Sensor Pod. This setting determines the units, scaling algorithm, and other settings that will be applied to the channel. More...
enum | BioPotentialChannelMode { BioPotentialChannelMode.Normal = 0x00, BioPotentialChannelMode.GSR = 0x01, BioPotentialChannelMode.TestSignal = 0x02, BioPotentialChannelMode.RIP = 0x03 }
| Describes the mode of operation set for a biopotential channel. More...
enum | BioPotentialTermination { BioPotentialTermination.SingleEnded, BioPotentialTermination.Differential }
| Specifies whether the BioRadio has been configured for Single-Ended or Differential inputs. When configured for differential inputs, 4 BioPotential channels are available. Otherwise, 8 channels are available. More...
enum | CouplingType { CouplingType.AC = 0x01, CouplingType.DC = 0x00 }
| Describes the possible coupling types that could be configured for a biopotential channel. More...
enum | EventButtonPolarity { EventButtonPolarity.ActiveHigh, EventButtonPolarity.ActiveLow }
| Describes the polarity of the BioRadio event button. The default is ActiveHigh. More...
enum | TransitionSensitivity { TransitionSensitivity.Edge, TransitionSensitivity.Level }
| Indicates the transition sensitivity for the BioRadio event marker button. More...

## Enumeration Type Documentation

## ◆ AuxiliaryTransducerType

enum GLNeuroTech.Devices.BioRadio.Configuration.AuxiliaryTransducerType : ushort

strong

The list of transducers that can be selected for the Auxiliary port of a Sensor Pod. This setting determines the units, scaling algorithm, and other settings that will be applied to the channel.

Enumerator
BloodPressure |
FlowRate |
ForcePlate |
GripStrength |
Temperature |

## ◆ BioPotentialChannelMode

enum GLNeuroTech.Devices.BioRadio.Configuration.BioPotentialChannelMode

strong

Describes the mode of operation set for a biopotential channel.

Enumerator
Normal | Normal operation mode.
GSR | The channel is configured for reporting GSR data
TestSignal | Directs the device to generate a 1.98Hz square wave on this channel.
RIP | The channel is configured for reporting RIP data

## ◆ BioPotentialTermination

enum GLNeuroTech.Devices.BioRadio.Configuration.BioPotentialTermination

strong

Specifies whether the BioRadio has been configured for Single-Ended or Differential inputs. When configured for differential inputs, 4 BioPotential channels are available. Otherwise, 8 channels are available.

Enumerator
SingleEnded | BioRadio is configured for Single-ended inputs
Differential | BioRadio is configured for Differential inputs

## ◆ CouplingType

enum GLNeuroTech.Devices.BioRadio.Configuration.CouplingType

strong

Describes the possible coupling types that could be configured for a biopotential channel.

Enumerator
AC | The channel uses AC coupling
DC | The channel uses DC coupling

## ◆ EventButtonPolarity

enum GLNeuroTech.Devices.BioRadio.Configuration.EventButtonPolarity

strong

Describes the polarity of the BioRadio event button. The default is ActiveHigh.

Enumerator
ActiveHigh | The button is Active High. Its unpressed state will generate a 0 and its pressed state is represented by a 1.
ActiveLow | The button is Active Low. Its unpressed state will generate a 1 and its pressed state is represented by a 0.

## ◆ TransitionSensitivity

enum GLNeuroTech.Devices.BioRadio.Configuration.TransitionSensitivity

strong

Indicates the transition sensitivity for the BioRadio event marker button.

Edge will generate a brief pulse transition whenever a press or release is detected. A quick press of the button could generate two edges and thus two pulses. Level will report the state of the button, based on the EventButtonPolarity setting.

Enumerator
Edge | Edge transition is used. The channel generates momentary pulses on each press and release.
Level | Level transition is used. The channel reports the state of the button.