Bio Radio SDK - Xamarin Android: AuxiliaryTransducerTypes.cs File Reference

| Bio Radio SDK - Xamarin Android

Classes | Namespaces | Enumerations
AuxiliaryTransducerTypes.cs File Reference

## Classes

class | GLNeuroTech.Devices.BioRadio.Configuration.EnumHelper

## Namespaces

namespace | GLNeuroTech.Devices.BioRadio.Configuration

## Enumerations

enum

GLNeuroTech.Devices.BioRadio.Configuration.AuxiliaryTransducerType : ushort {
GLNeuroTech.Devices.BioRadio.Configuration.AuxiliaryTransducerType.BloodPressure = 0, GLNeuroTech.Devices.BioRadio.Configuration.AuxiliaryTransducerType.FlowRate = 1, GLNeuroTech.Devices.BioRadio.Configuration.AuxiliaryTransducerType.ForcePlate = 2, GLNeuroTech.Devices.BioRadio.Configuration.AuxiliaryTransducerType.GripStrength = 3,
GLNeuroTech.Devices.BioRadio.Configuration.AuxiliaryTransducerType.Temperature = 4
}

| The list of transducers that can be selected for the Auxiliary port of a Sensor Pod. This setting determines the units, scaling algorithm, and other settings that will be applied to the channel. More...